< Film over error for the upper (461)

Error content | Film over error for the upper.
Detail | When upper film was sending, the film detection board for film over was fallen down. Sub-error meanings are as follows: 0001: During the film centering. 0002: Performing unloaded feeding. 0003: During the film feeding.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part |
Remarks | Remove film after recovery operation. <Points to be checked> 嘆 P-1105 [A200] 嘇 Before the film over detection [B209]. 嘊 After the film over detection [B211].