< Automatic label length adjustment (1861-1000)

Error content | Displayed pressing [AUTO LNG. ADJUST] button on LABEL APPLICATOR (LABEL) screen.
Detail | Confirm to execute the automatic label length adjustment.
Solution | Press [EXEC] or [STOP] button. [EXEC]: Head check is performed to the next product. [STOP]: Head check is not performed to the next product.
Action by user | Press [EXEC] or [STOP] button.
Action by service representative
Related part |
Remarks | Only for POP printer.