< Lift change is abnormal (423)

Error content | Lift change error.
Detail | Lift change operation did not finish normally. Sub-error meanings are as follows: 0003: Changeover sensor is not receiving light when lowering the lift. 0010: Operation wasn乫t completed during changing to small lift. 0011: Operation wasn乫t completed during the changing to large lift.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Lift change solenoid position [B214] 嘊 Lift change solenoid [L200]
Remarks |