- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No response from applicator (602)

Error content | No response has been received from the label applicator in a case other than the power-on notification when power is turned on.
Detail | ・Communication between the main unit and the label applicator has not been performed. ・The sub-error includes the communication phase number. ・A communication error immediately after the completion of power-on processing will cause this error.
Solution | Press [STOP] to disconnect the communication with the label applicator. Operation is possible without label applicator. Press the [REEXEC] button to check the connection with the label applicator. Release the error after confirming the connection.
User’s action |
Service person’s action |
Relevant locations | P-1105 [A100] (Disconnection of the connector XJ-21)
Remarks | Operation is possible without label applicator operation after the [STOP] button is pressed.