- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Cutter is not back to original position (481)

Error content | Cutter is not back to original position.
Detail | Cutter is not back to original position when starting cutter operation.
Solution | Press the [RETURN] button after checking for objects.
Action by user |
Action by service representative |
Related part | ① P-1105 [A300] ② Origin point of cutter [B300]. ③ Cutter solenoid front [L300]. ④ Cutter solenoid rear [L301].
Remarks |