< No label to apply (610)

Error content | No label to apply.
Detail | There was no label when application was attempted. Sub-error meanings are as follows: 0000: Applicator failed in labeled absorption.
Solution | [RETURN] button
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor.
Related part | 嘆 P-1105 [A100] 嘇 P-1006 [A101] 嘊 Label presence [B116] 嘋 Label suction fan [M107]
Remarks |