n It could not suck POP label (609-2000)

Error content | Applicator failed in label application.
Detail | Sub-error meaning is as follows: 2000: POP applicator failed in labeled absorption.
Solution | Press [RETURN] or [PLU] button then the indication releases automatically.
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor. Adjust the issue position by printing adjustment. Adjust the suction position on the printer adjustment screen.
Related part | (1) P-1105 [A100] (2) P-1006 [A101] (3) Label presence [B116] (4) Label suction fan [M107]
Remarks |