n Thermal head for printer 1 up (716-0001, 816-0001, 1016-0001)

Error content | Thermal head for printer 1 up.
Detail | The thermal head was up when printing starts. This error is displayed in DP mode.
Solution | Press [OK] button after setting the thermal head.
Action by user |
Action by service representative |
Related part |
Remarks | Printer number is changed depending on error number. Illustration of indicator is displayed by type of models.