n Abnormal for applicator (POP) (615-2000)

Error content | Error occurred during application operation.
Detail | Operation was not completed within the set time during motor operation. Sub-error meanings are as follows: 200*: X axis (* = 0: moving left, 1: moving right) 202*: Z axis (* = 0: moving up, 1: moving down) 203*: 兤 axis (* = 0: rotating to right, 1: rotating to left)
Solution | Press [RETURN] button.
Action by user | Check if the applicator can be moved smoothly with hands while the emergency stop switch is being pressed.
Action by service representative | Check the grease condition.
Related part | <X axis> (1) P-1105 [A100] (2) P-1006 [A102] (3) X axis motor [M103] (4) X axis origin point [B108] <Z axis> (1) P-1105 [A100] (2) P-1006 [A101], [102] (3) Z axis motor [M105] (4) Z axis origin point [B112] <兤 axis> (1) P-1105 [A100] (2) P-1006 [A101] (3) 兤-axis motor [M106] (4) Below 兤-axis detection board [B113] (5) Above 兤-axis detection board [B114]
Remarks |