< Heater safety guard is up (484)

Error content | Heater safety guard is up.
Detail | After the pusher is restored, if the heater safety guard is up, the pusher downs the guard. If the sensor is still emitted afterwards, an error occurs.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A100] 嘇 Origin point of heater safety guard [B103]. 嘊 Heater safety guard solenoid [L100].
Remarks |