- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Do not put your hands into the machine (448)

Error content | A hand was put into the wrapper during operation.
Detail | Occurs when a hand or object is detected entering the infeed conveyor while the wrapper is operating. 0000: A hand is detected entering the infeed conveyor in forward side. 0001: A hand is detected entering the infeed conveyor in backward side
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Hand insertion in the infeed conveyor <forward side> (light receiving/emitting) [B216]. ③ Hand insertion in the infeed conveyor <backward side> (light receiving/emitting) [B215].
Remarks |