- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■Abnormal for applicator (POP) (615-2000)

Error content | Error occurred during application operation.
Detail | Operation was not completed within the set time during motor operation. Sub-error meanings are as follows: 200*: X axis (* = 0: moving left, 1: moving right) 202*: Z axis (* = 0: moving up, 1: moving down) 203*: θ axis (* = 0: rotating to right, 1: rotating to left)
Solution | Touch [RETURN] button.
Action by user | Check if the applicator can be moved smoothly with hands while the emergency stop switch is being pressed.
Action by service representative | Check the grease condition.
Related part |
<X axis> | <Z axis> | <θ axis>
--- | --- | ---
① P-1105【A400】 ② P-1006【A402】 ③ X axis motor【M400】 ④ X axis origin point【B407】 | ① P-1105【A400】 ② P-1006【A401】【A402】 ③ Z axis motor【M401】 ④ Z axis origin point【B401】 | ① P-1105【A400】 ② P-1006【A401】 ③ θ axis motor【M402】 ④ θ axis origin point【B402】 ⑤ Above θ axis detection board【B403】
Remarks |