- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Lift change is abnormal (423)

Error content | The lift changing solenoid is abnormal.
Detail | The lift changing solenoid operation has not been completed normally. The sub-error has the following meanings: 0003: The changing sensor is light-shielded when the lift starts descending. (Past instance: The returning spring coil was cut.) 0010: The operation is not completed while changing to the small lift. 0011: The operation is not completed while changing to the big lift. Error that occurs when Sensor B214 is not light-shielded when the solenoid is pulled. (This is not the Big lift B201 confirmation sensor error.)
Solution | Press the [RETURN] button.
User’s action | Press [RETURN] button to release the error.
Service person’s action | Check the following related parts and repair or replace the defective part(s).
Relevant locations | ① P-1105 [A200] ② Lift changing solenoid position sensor [B214] ③ Lift changing solenoid [L200] ④ Lift changing spring coil
Remarks |