< Motor for R/L squeeze is abnormal (416)

Error content | Motor for R/L squeeze error.
Detail | Motor for R/L squeeze operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0011: The origin sensor is not receiving light at the timing with the origin sensor not receiving light.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A100] 嘇 Driving motor for R/L squeeze [M03] 嘊 Origin point of R/L squeeze [B102]
Remarks |