- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Left film remove cover is open (0307)

Error content | Left film remove cover is open.
Detail | Occurs when the left film remove cover is open before operation.
Solution | Close left film remove cover, [OK] button.
Action by user | Close the film removal door on the left.
Action by service representative | Close the film removal door on the left.
Related part | Main board, wrapping machine board
Remarks |