- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Lower film has overrun (462)

Error content | Lower film overrun error.
Detail | The film overrun detection plate fell down when the lower film was fed. Sub-error meanings are as follows: 0001: At the time of film centering. 0002: At the time of idling operation. 0003: At the time of film feeding.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Film overrun detection (front) [B209] ③ Film overrun detection (rear) [B211]
Remarks | The film needs to be removed after performing return processing.