- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< There is problem on wrapping controller (472)

Error content | The slave board for wiring-saving of the wrapper is abnormal.
Detail | A communication error has occurred between the parent device (P-1105: A200 lower right) of the wrapper control board and the child device (P-1105: A100 upper left, A300 lower left). The sub-error has the following meanings: <Without POP printer> 0000: Communications between both A200 and A100, A200 and A300 are abnormal. 0001: Communication between A200 and A300 is abnormal. 0002: Communication between A200 and A100 is abnormal. <With POP printer> 0000: Communications all between A200 and A100, A200 and A300, A200 and A400 are abnormal. 0001: Communications both between A200 and A300, A200 and A400 are abnormal. 0002: Communications both between A200 and A100, A200 and A400 are abnormal. 0003: Communication between A200 and A400 is abnormal. 0004: Communications both between A200 and A100, A200 and A300 are abnormal. 0005: Communication between A200 and A300 is abnormal. 0006: Communication between A200 and A100 is abnormal. The following CAN communication has not been established: P-1105 [A100] (XJ5) - P-1105 [A300] XJ4 P-1105 [A300] (XJ5) - P-1105 [A200] XJ5 The harness is sequentially connected to the main board A10 upper right → A300 upper left → A100 lower left → A200 lower right (A400 lower right for POP), but communication is conducted from A200. It is possible that the RS485 communication is abnormal. Short-circuiting of XJ7 is used for the board number recognition. In case of this error, the RS485 communication between P-1163 and P-1105 A200 is established. This means that RS485 and CAN harnesses are not disconnected. However, disconnection may occur between P-1105 [A200] and P-1105 [A400] when a POP printer is connected.
Solution | Turn on the power again.
User’s action |
Service person’s action |
Relevant locations | ① P-1105 [A100], [A200], [A300] ② Pin 23 and Pin 24 at XJ7 of P-1105 [A100] should be short circuited. ③ Pin 21 and Pin 22 at XJ7 of P-1105 [A200] should be short circuited. ④ Pin 21 and Pin 22 and Pin 23 and Pin 24 at XJ7 of P-1105 [A100] should be short circuited.
Remarks | First, confirm that XJ7 of each board is connected. When all are connected, there is a high probability that the board is defective. This has nothing to do with software. (A different error will occur if the software is not installed.)