- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Automatic adjustment cannot be completed (1537)

Error content | Automatic adjustment for the detector failed.
Detail | The detector could not successfully complete the automatic adjustment. Which automatic adjustment caused the error is separated by sub-error No. 0000: brightness adjustment failed 0001: distortion adjustment failed 0002: volume adjustment failed
Solution | [OK] button
Action by user |
Action by service representative | Sub-error No.: [0000] and [0001] Perform automatic adjustment of brightness and distortion after confirming the detector board and LED light for tray detection. If failed, manually perform adjustment of the detector. Sub-error No.: [0002] Perform volume height automatic adjustment after confirming the volume height sensor.
Related part | Detector board [A221] LED light for tray detection. Volume height detection sensor.
Remarks | When automatic adjustment fails, the adjustment value returns to the value before the execution.