< Insert plate is not back to original position (482)

Error content | Insert plate is not back to original position.
Detail | The cutter can't be switched on as the insert plate has not returned to its original position when cutter operation started. Sub-error meanings are as follows: 0000: Upper side insert plate did not return to its original position. 0001: Lower side insert plate did not return to its original position. 0006: Insert plate of send side did not return to its original position during returning operation. 0007: Insert plate did not return to its original position while loading.
Solution | Press the [RETURN] button after checking the insert plate.
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 Origin point of insert [B301].
Remarks |