< Bracket for camera is up (0310)

Error content | Bracket for camera is up.
Detail | Camera is pushed up when production.
Solution | Back the camera to the original position, [OK] button.
Action by user | Put the camera back to the original position. Press the [OK] button
Action by service representative | Put the camera back to the original position.
Related part | Main board, wrapping machine board
Remarks |