- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Bracket for camera is up (0310)

Error content | Bracket for camera is up.
Detail | Camera is pushed up when production.
Solution | Back the camera to the original position, [OK] button.
Action by user | Put the camera back to the original position. Press the [OK] button
Action by service representative | Put the camera back to the original position.
Related part | Main board, wrapping machine board
Remarks |