- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

Error Number | Error Content
--- | ---
Normal | W type | P type
No.1 00700 First | No.2 00800 Second | No.4 01000 Bottom label | No.5 01900 POP label
00703 | 00803 | 01003 | - | Printer * has problem
00704 | 00804 | 01004 | - | Printer * has problem
00707 | 00807 | 01007 | - | Printer * is not initialized
00710 | 00810 | 01010 | - | No label for printer * (0001)
00710 | 00810 | 01010 | - | No label for printer * (0002)
00711 | 00811 | 01011 | 01911 | Label size error for printer * (0001)
00711 | 00811 | 01011 | - | Label size error for printer * (0002)
00713 | 00813 | 01013 | - | Too many characters on format for printer *
- | - | 01014 | - | Label Remaining on Underlabeller
00715 | 00815 | 01015 | - | Thermal head is worn out for printer *
00716 | 00816 | 01016 | - | Thermal head for printer * up(0001)
00716 | 00816 | 01016 | - | Thermal head for printer * up(0002)
00717 | 00817 | 01017 | 01917 | Control board for printer * is failed
- | - | - | 01967 | POP printer cover is not set
- | - | 01040 | - | Cutter cover is not set
- | - | 01068 | - | Cutter cover is not set
- | - | 01069 | - | Cutter error
- | - | 01070 | - | Label is jammed at cutter unit
- | - | 01088 | - | Cutter original position error