n No POP label to apply (610-2000)

Error content | No label to apply.
Detail | There was no label when application was attempted. Sub-error meaning is as follows: 2000: Standard applicator failed in label absorption.
Solution | Press [RETURN] button.
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor.
Related part | (1) P-1105 [A100] (2) P-1006 [A101] (3) Label presence [B116] (4) Label suction fan [M107]
Remarks |