- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Shutter operation of PS-AI is abnormal (526)

Error content | The shutter operation of PS-AI is abnormal.
Detail | The origin sensor did not properly receive or block light in the PS-AI's shutter operation. The sub-error has the following meanings: 0001: The right side of the original position of the shutter was in a light-shielded state when the shutter came out. 0002: The left side of the original position of the shutter was in a light-shielded state when the shutter came out. 0003: Both right and left sides of the original position of the shutter were in a light-shielded state when the shutter came out. 0010: Both right and left sides of the original position of the shutter were in a floodlighted state when the shutter was returned to its original position. 0011: The left side of the original position of the shutter was in a floodlighted state when the shutter was returned to its original position. 0012: The right side of the original position of the shutter was in a floodlighted state when the shutter was returned to its original position. (The ones digit indicates the status of the origin sensor)
Release method |
User’s action | When using the shutter continuously, press the [EXEC] button to perform the recovery operation. After that, when canceling the shutter operation, press the [STOP] button to resume operation. (The shutter operation is not performed until the power is turned off)
Service action |
Relevant locations | 1) P-1105[A600] 2) Shutter solenoid 1 (driver) [L603] [E604] 3) Shutter solenoid 2 (driver) [L604] [E605] 4) Shutter original position (right) [B612] 5) Shutter original position (left) [B613]
Remarks |