< Thermal head for printer 1 up (716-0002, 816-0002)

Error content | Thermal head for printer 1 up.
Detail | The thermal head was up when printing starts. This error is displayed when closing the front cover.
Solution | Press the [RETURN] button after setting the thermal head.
Action by user |
Action by service representative |
Related part |
Remarks | 乬Printer No.1乭 changes depending on error No.