- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Control board for printer 1 is failed (717-****, 817-****,1017-****,1917-****)

0717-**** | The control board of Printer 1 is abnormal. | First top label printer
0817-**** | The control board of Printer 2 is abnormal. | Second top label printer
1017-**** | The control board of Printer 4 is abnormal. | Bottom label printer
1917-**** | The control board of Printer 5 is abnormal. | POP printer

Error content | Abnormality of the printer control board (Printer 1: P-1100, Printer 2: P-1001, POP label printer: P-1131, Bottom label printer: P-1131)
Detail | Unable to detect an interrupt signal from the printer control board (P-1163, P-1001, P-1131). Sub-error "0001" occurs when the front cover is open in DP mode.
Solution | Restore power
Action by user | Restore power
Action by service representative | Printer 1, Printer 2 CCheck the communication harness between P-1100 (XJ25) and P-1001 (XJ18) Check for poor connector contact POP label printer, Bottom label printer Check the USB communication cable. Replace the printer control board (Printer 1: P-1100, Printer 2: P-1001, POP label printer: P-1131, Bottom label printer: P-1131)
Related part |
Remarks | “Printer No.1” changes depending on error No.