< Motor for film change is abnormal (412)

Error content | Motor for film change error.
Detail | Motor for film change operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0011, 12: The origin point of film 2 change [B309] is not receiving light at the timing not to receive light. 0020: The origin point of film 1 change [B304] and the origin point of film 2 change [B309] are receiving light when the insert operation or change operation start.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 P-1006 [A301] 嘊 Stepping motor for film change [M304] 嘋 Origin point of film 1 change [B304], origin point of film 2 change [B309]
Remarks |