- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

<Auto feeder is not connected (0395)

Error content | Auto infeeder is not connected
Detail | This error occurs when an operation request is received while PS-AI is disconnected.
Solution | Press the [OK] button.
Action by user | Confirm the connection point (key switch) with PS-AI, then press the [OK] button.
Action by service representative | Confirm the connection point (key switch) with PS-AI, then press the [OK] button.
Related part | Main board, wrapping machine board
Remarks |