< Film loading was failed on the upper (467)

Error content | Film loading was failed on the upper.
Detail | Film transport could not compete successfully in film loading operation because send film detection board did not fall down in right order. Sub-error meanings are as follows: 0000: upper film loading failed. 0001: Lower film loading failed.
Solution | Press the [RETURN] button after removing the remaining film on the side blinking blue.
Action by user |
Action by service representative |
Related part |
Remarks | The error will not be displayed by selection [No] in film error machine settings.