< Motor for back squeeze plate is abnormal (415)

Error content | Motor for back squeeze plate error.
Detail | Motor for back squeeze plate operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0011: The origin sensor is not receiving light at the timing with the origin sensor not receiving light.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A100] 嘇 Driving motor for back squeeze plate [M02] 嘊 Origin point of back squeeze plate [B101]
Remarks |