- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Feeder bar is not original position (477)

Error content | Feeder bar is not original position.
Detail | The feeder bar was not in its original position when the wrapper started feeder operations (excluding return operation).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Origin point of feeder bar [B204].
Remarks |