- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n No label for under labeller (1010-0002)

Error content | Printer label is run out.
Detail | In the state that the front cover is closed and the under labeller unit set, displays when labels have run out at the time of the label issuing.
Solution | Pull the under labeller unit out and perform unloaded feed after replacing the label, setting the under labeller unit, then press [RETURN] or [PLU] button.
Action by user |
Action by service representative |
Related part |
Remarks |