- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Feed bar motor is abnormal (421)

Error content | Feeding bar motor error
Detail | The feeding bar motor operation has not been completed normally. The sub-error has the following meanings: 0001: The operation is not completed though the operation protection timer has expired. 0003: The DCB motor is overloaded. 0004: The feedback pulse from the DCB motor is abnormal (phase interruption). 0013: The DCB motor at the reversal operation is overloaded. (Reversal operation = Performed when the return operation is performed or at the end of the feeding operation.) 0999: Back-feed exceeding the limit count is performed. 1000 or above: The motor steps out. The value indicates a rough position in which the stepping out of the motor was detected.
Solution | Press the [RETURN] button.
User’s action | Pres [RETURN] button to release the error.
Service person’s action | Check the following related parts and repair or replace the defective part(s).
Related part | ① P-1105 [A200] ② Feeding bar motor [M04] ③ Feeding bar origin [B204] ④ Feeding plastic container chain, feeding bar (right and left, small bearings), sprocket bearings, Right and left guide pushers ⑤ Driving chain (Chain between the motor and the shaft)
Remarks |