- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Problem on wrapping part (498)

Error content | The wrapper system is abnormal.
Detail | Something was wrong with the wrapper program. The sub-error has the following meanings: 001X to 003X: Synchronization deviation of CAN communication. 0012: Only the child device (A100) accepts a command to the wrapping request / No response is received for the hold instruction transmission. 0013: Only the child device (A100) accepts a command to the discharge request / No response is received for the hold instruction transmission. 0017: Only the child device (A100) accepts a command to the wrapping request / A response different from the transmission is returned for the hold instruction transmission. (Past instance: This error occurred when the right/left squeezing original position sensor failed due to contact with the detection plate.) 0018: Only the child device (A100) accepts a command to the discharge request / A response different from the transmission is returned for the hold instruction transmission. 0022: Only the child device (A100) accepts a command to the wrapping request / No response is received for the hold instruction transmission. 0023: Only the child device (A100) accepts a command to the discharge request / No response is received for the hold instruction transmission. 0027: Only the child device (A100) accepts a command to the wrapping request / A response different from the transmission is returned for the hold instruction transmission. (Past instance: This error occurred when the holding bar encoder sensor failed due to contact with the detection plate.) 0028: Only the child device (A100) accepts a command to the discharge request / A response different from the transmission is returned for the hold instruction transmission. 0032: Both the child device (A100) and the child device (A300) accept a command to the wrapping request / No response is received for the hold instruction transmission. 0033: Both the child device (A100) and the child device (A300) accept a command to the discharge request / No response is received for the hold instruction transmission. 0037: Both the child device (A100) and the child device (A300) accept a command to the wrapping request / A response different from the transmission is returned for the hold instruction transmission. 0038: Both the child device (A100) and the child device (A300) accept a command to the discharge request / A response different from the transmission is returned for the hold instruction transmission. 1014: The operation is not completed though the pinching operation protection timer has expired. 1017: The operation is not completed though the cutter operation protection timer has expired.
Solution | Turn on the power again.
User’s action |
Service person’s action | CAN communication error (XJ11 and XJ12 on each board) Sub-code 0017 when A100 fails Sub-code 0027 when A300 fails 0402-**** appears because communication cannot be made with the main board when A200 fails. This error often occurs due to sensor failure from past instances. Check when this error occurs by pulling out any wire other than wires necessary for communication (XJ4, 5, 7, 26, 27) of P-1105.
Related part | XJ4 and XJ5 on each board of P-1105 [A100, A200, A300] Various sensors
Remarks | This error is determined by P-1105 [A200], and the error code is transmitted to the main board [A10] through the RS485 communication.