- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film over error for the upper (461)

Error content | Film over error for the upper.
Detail | When upper film was sending, the film detection board for film over was fallen down. Sub-error meanings are as follows: 0001: During the film centering. 0002: Performing unloaded feeding. 0003: During the film feeding.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part |
Remarks | Remove film after recovery operation. <Points to be checked> ① P-1105 [A200] ② Before the film over detection [B209]. ③ After the film over detection [B211].