< Film driving motor is abnormal (413)

Error content | Film driving motor error.
Detail | Film driving (right) motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 Film driving motor [M08]
Remarks |