- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film loading was failed on the upper (467)

Error content | Film loading was failed on the upper.
Detail | Film transport could not compete successfully in film loading operation because send film detection board did not fall down in right order. Sub-error meanings are as follows: 0000: upper film loading failed. 0001: Lower film loading failed.
Solution | Press the [RETURN] button after removing the remaining film on the side blinking blue.
Action by user |
Action by service representative |
Related part |
Remarks | The error will not be displayed by selection [No] in film error machine settings.