- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Abnormal for applicator (615)

Error content | The label applicator operation is abnormal.
Detail | During operation of the motor, the operation has not been completed within the prescribed time. The sub-error has the following meanings: 000*: X axis (* = 0: When moving to the left, 1: When moving to the right) 001*: Y axis (* = 0: When moving in the forward direction, 1: When moving in the backward direction) 002*: Z axis (* = 0: When ascending, 1: When descending) 003*: θ axis (* = 0: When rotating clockwise, 1: When rotating counterclockwise) 013*: The sensor event is not generated even after the elapse of the prescribed time when performing the θ axis (* = 0: When rotating clockwise, 1: When rotating counterclockwise) correction operation. 0100: The label applicator moves in front of Printer 2 although Printer 1 is in the sucking state. 0101: The label applicator moves in front of Printer1 although Printer 2 is in the sucking state.
Solution | Press the [RETURN] button.
User’s action | Confirm that the label applicator can be moved smoothly by hand while the emergency stop button is pushed.
Service person’s action | Check the state of grease.
Related part | <In the case of X axis> ① P-1105 [A100] ② P-1006 [A102] ③ X-axis motor [M103] ④ X-axis origin [B108] ⑤ Printer 1 position [B109] ⑥ Printer 2 position [B110] <In the case of Y axis> ① P-1105 [A100] ② P-1006 [A101] ③ Y-axis motor [M104] ④ Y-axis origin [B111] <In the case of Z axis> ① P-1105 [A100] ② P-1006 [A101], [A102] ③ Z-axis motor [M105] ④ Z-axis origin [B112] <In the case of θ axis> ① P-1105 [A100] ② P-1006 [A101] ③ q-axis motor [M106] ④ Lower θ-axis detection plate [B113] ⑤ Upper θ-axis detection plate [B114] In the case of “0615-0021” is displayed ・Defects in the changing power supply of the label applicator unit U101 ・P-1105 [A100] (Disconnection of the connector XJ-20) When the “0422-0001” error is displayed immediately after “0615-0021” is displayed. ・F104 or F105 fuse may be disconnected.
Remarks |