< Left film remove cover is open (0307)

Error content | Left film remove cover is open.
Detail | Occurs when the left film remove cover is open before operation.
Solution | Close left film remove cover, [OK] button.
Action by user | Close the film removal door on the left.
Action by service representative | Close the film removal door on the left.
Related part | Main board, wrapping machine board
Remarks |