- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■Label Remaining on Underlabeller (01014-0003)

Error content | Label Remaining on Underlabeller.
Detail | Displayed when pasting bottom label fails.
Solution | Touch [Remove] button.
Action by user | Touch [Remove] button, then remove the issued label. If the label is not automatically ejected, pull out the bottom label printer unit and check if there is any label left on the label transport unit or cutter unit of the printer. Remove the label when it remains.
Action by service representative | Check the peeling sensor and the label transport unit sensor.
Related part | Bottom label printer board
Remarks | Bottom label printer (Printer 4) dedicated error