- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n It could not suck POP label (609-2000)

Error content | Applicator failed in label application.
Detail | Sub-error meaning is as follows: 2000: POP applicator failed in labeled absorption.
Solution | Press [RETURN] or [PLU] button then the indication releases automatically.
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor. Adjust the issue position by printing adjustment. Adjust the suction position on the printer adjustment screen.
Related part | (1) P-1105 [A100] (2) P-1006 [A101] (3) Label presence [B116] (4) Label suction fan [M107]
Remarks |