< Sensor for the back side of feeder is abnormal (483)

Error content | Sensor for the back side of feeder is abnormal.
Detail | An impossible input combination has occurred in the sensor (Original point, small lift boundary, large lift boundary) detecting the back feeder position. The sub-error screens the input conditions as shown below. 0003: Original point and the small lift boundary sensor are not receiving light. 0005: The small lift boundary sensor and the large lift boundary sensor are not receiving light. 0006: The original point sensor and the large lift boundary sensor are not receiving light. 0007: Three of them are not receiving light.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Back side of feeder, origin point [B212]. 嘊 Back side of feeder, position small [B217]. 嘋 Back side of feeder, position large [B218].
Remarks |