< Film heater has problem (426)

Error content | Film heater error.
Detail | As an error occurs in film heater, unable to use the heater. Sub-error meanings are as follows: 0001: Thermistor of film heater is disconnected. 0100: A fan alarm occurs (alarm also occurs when connector is not inserted).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 Thermistor for film heater [R300] 嘊 Fan for film heater [M305]: Sub-error is 100
Remarks | After the error occurrence, unable to use the left side film heater.