< Cannot connect with camera unit (1506)

Error content | Unable to communicate between tray detector and the tray detector camera.
Detail | It has been decided that the camera is not connected due to the inability to obtain a proper response when attempting to set the camera.
Solution | [OK] button => Operate without the tray detector. (Operate with registered trays.)
Action by user |
Action by service representative | Confirm the connection between the detector board and CMOS camera [A221 XJ-4].
Related part | Detector board (P-1107) [A221] CMOS camera
Remarks |