- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Blackout for the power (1504)

Error content | Tray detector detected power OFF in the console.
Detail | Power ON command received twice from the console.
Solution | Restore power
Action by user |
Action by service representative | Confirm the power supply 24 V DC of the main board (P-1100, P-1163, P-1000). RS485 communication line of the main board [A221 XJ-11].
Related part | Switching power supply [U10] Main board (P-1100, P-1163, P-1000) [A10] Detector board (P-1107) [A221]
Remarks |