- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Lift motor is abnormal (410)

Error content | Lift motor is abnormal
Detail | Lift motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn't completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0101: The lower side of lift [B203] is not receiving light, when lowering the lift. 0102: The lower side of lift [B203] is emitted light, after switching or returning the lift. 0103: The origin point of lift [B202] and the lift safety [B204] are not receiving light. when the lift backs to its origin point. 0104: The origin point of lift [B202] and the lift safety [B204] are not receiving light when the lift is in its switch position. 0105: The origin point of lift [B202] is not receiving light when lowering the lift. The lift lower side position [B203] is emitted light wen the lift backs to its origin point. 0106: Do not block light of the lift origin point [B200] when the lift is moving to the origin point after the lift changeover. 0107: The lift origin point [B200] is not receiving light when lowering the lift. 0201: The lift origin point [B200] is not receiving light even after a certain period of time after the lift starts operation.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Motor for lift [M06] ③ Sensors described above: [B200], [B202], [B203], [B204]
Remarks |