- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Label is remaining on applicator (0312-0001)

Error content | Label is remaining. A label remains at the label applicator. It is detected by the same sensor as in the case of Error 0351.
Detail | The content can be segmented by the sub-error number. 0000: Printer The peeling sensor is shielded from light when prechecking the start of printing. The peeling sensor value (Peel Sensitivity) is less than the threshold value (Peel Detect). Adjust the peeling sensor sensitivity. Check that the optical axis of the peeling sensor is positioned accurately. The message may vary depending on the error location. 0001: Label applicator (The label detection sensor is in a reflection state, and the error is detected by the sensor check of the upper label applicator.) 0002: POP label applicator
Release method | Remove the label remaining at the printer and press the [OK] button.
User’s action | Remove the label remaining at the printer and adjust slackning of the label mount. Remove the label remaining at the label applicator.
Service action | Check the operation of the peeling sensor of the printer that has caused an error. Check the label detection sensor of the label applicator (upper label applicator sensor check).
Relevant locations | Printer #1: Main board P-1100, Peeling sensor Printer #2: Printer board P-1101, Peeling sensor Label applicator: Wrapping board P-1105 [A100] (upper left) XJ-20, P-1006-5 [A101] XJ-5 and 7, Label detection sensor, Curl cord, Movable harness POP label applicator: Wrapping board P-1105 [A400] (upper right) XJ-20, P-1006-5 [A401] XJ5 and 7, Label detection sensor, Curl cord, Movable harness
Remarks | Error 0312: Error that occurs when a label is detected during the precheck before operation Error 0351: Error that occurs when the remaining label error display time is set.