< Feed bar motor is abnormal (421)

Error content | Feed bar motor error.
Detail | Feed bar motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0999: Back feed was performed exceeding the count limit. 1000 or above: Motor was stepped out. The value indicates approximate location where stepping out was detected.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Feed bar motor [M04] 嘊 Origin point of feed bar [B204]
Remarks |