- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Motor for film feed is abnormal (411)

Error content | Motor for film feed is abnormal.
Detail | Film insert motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn’t completed when the operation protection timer run out. 0011: The insert motor was stepped out when the film is traveling. 0021: The insert didn’t back to the normal position when the cutter starts operation.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A300] ② P-1006 [A301] ③ Stepping motor for film feed [M303] ④ Film feed origin point [B301]
Remarks |