- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Heater safety guard is up (484)

Error content | Heater safety guard is up.
Detail | After the pusher is restored, if the heater safety guard is up, the pusher downs the guard. If the sensor is still emitted afterwards, an error occurs.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A100] ② Origin point of heater safety guard [B103]. ③ Heater safety guard solenoid [L100].
Remarks |